┌────────────────────────────────────────────────────────────────────┐

│ • MobaXterm 10.9 • │

│ (SSH client, X-server and networking tools) │

│ │

│ ➤ Telnet session to 192.168.0.250 │

│ ➤ Your DISPLAY is set to 192.168.0.10:0.0 │

│ ➤ For more info, ctrl+click on help or visit our website │

└────────────────────────────────────────────────────────────────────┘

(none) login: root

Password:

BusyBox v1.1.2 (2009.12.19-18:27+0000) Built-in shell (ash)

Enter 'help' for a list of built-in commands.

Welcome to HiLinux.

None of nfsroot found in cmdline.

~ $ vi config.ini

portnum=65001

ipadd=47.94.44.231

device\_id=01016000

station\_id=01015000

HEARTBEAT=30

DEBUG=1

CRYPT=1

WEIDU=45681641

JINGDU=126709557

funa=6205

funb=119

func=11500

RADAR\_PARAMENT=101

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

- config.ini [modified] 1/13 7%

portnum=65001

ipadd=47.94.44.231

device\_id=01016000

station\_id=01015000

HEARTBEAT=30

DEBUG=1

CRYPT=1

WEIDU=45681641

JINGDU=126709557

funa=6205

funb=119

func=11500

RADAR\_PARAMENT=101

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

- config.ini [modified] 1/13 7%

portnum=65001

ipadd=47.94.44.231

device\_id=01016000

station\_id=01015000

HEARTBEAT=30

DEBUG=1

CRYPT=1

WEIDU=45681641

JINGDU=126709557

funa=6205

funb=119

func=11500

RADAR\_PARAMENT=101

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~

~ $ ./taxier

value\_access = 0

打开数据库

portnum = 65001

ipadd = 47.94.44.231

device\_id is = 01016000 device\_id\_hex is = 30

device\_id\_hex is = 31

device\_id\_hex is = 30

device\_id\_hex is = 31

device\_id\_hex is = 36

device\_id\_hex is = 30

device\_id\_hex is = 30

device\_id\_hex is = 30

station\_id is = 01015000

station\_id is = 01

station\_id is = 01

station\_id is = 50

station\_id is = 00

DEBUG = 1

CRYPT= 1

floor\_value = 0

WEIDU = 45681641

JINGDU = 126709557

funa = 62.050000

funb = 1.190000

func = 115.000000

HEARTBEAT = 30

RADAR\_PARAMENT = 101

open /dev/ttyAMA1

open\_uart success

init is OK

end of openfile

enter save\_msg\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

enter send\_msg \*\*\*\*\*\*\*\*\*\*\*

enter rec\_ask \*\*\*\*\*\*\*\*\*\*\*

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 //车辆信息标识

32 95 98 //起始设备ID编码

00 03 98 //目的设备ID编码

d0 c1 35 cc //流水号

00 75 //帧字节长度

00 00 //CRC校验

40 //帧类型

19 03 29 15 06 56 //当前本地时间（压缩BCD码YYMMDDhhmmss）

41 4c 30 30 30 35 00 //车辆编号（0x00结尾字符串）

35 39 c2 b7 00 //线路信息（0x00结尾字符串）

c9 cf d0 d0 00 //服务信息（0x00结尾字符串）

00 //司机信息（0x00结尾字符串）<这里没有司机信息>

34 35 2e 36 38 32 32 36 36 4e | 2c | 31 32 36 2e 37 31 30 34 31 39 45 | 2c | 30 | 2c | 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 36 3a 35 36 | 2c | 34 2e 36 31 33 33 33 32 | 2c | 33 37 2e 39 00 //定位信息（0x00结尾字符串，表示如下：1.纬度,经度,高程,时间,速度,方向；2.分隔符为半角< 分隔符为0x2c >）

ba cd d0 cb c2 b7 00 //站台信息（0x00结尾字符串）

34 2e 36 31 33 33 33 32 00 //行驶速度（0x00结尾字符串）

00 //行驶方向

02 //客流负载

03 //运行状态

02 //与前车间距

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = -1

rssibuff[26][-1] = 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 bb 03 98 bc 03 98 bb 03 98 b8

RSSI EE recived from uart

queueNo is -1

queueno=-1 new id : 03 98

queueNo=-1 rssi=72.000000 dist=25 return=25

queueNo=-1,03,98

queueNo=-1 8=03,9=03

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 ce 00 75 00 00 40 19 03 29 15 07 05 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 34 39 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 30 35 2c 30 2e 35 35 33 37 34 38 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 35 35 33 37 34 38 00 00 02 03 02

信息解析：

09 //车辆信息标识

32 95 98 //起始设备ID编码

00 03 98 //目的设备ID编码

d0 c1 35 ce //流水号

00 75 //帧字节长度

00 00 //CRC校验

40 //帧类型

19 03 29 15 07 05 //当前本地时间（压缩BCD码YYMMDDhhmmss）

41 4c 30 30 30 35 00 //车辆编号（0x00结尾字符串）

35 39 c2 b7 00 //线路信息（0x00结尾字符串）

c9 cf d0 d0 00 //服务信息（0x00结尾字符串）

00 //司机信息（0x00结尾字符串）<这里没有司机信息>

34 35 2e 36 38 32 32 39 33 4e | 2c | 31 32 36 2e 37 31 30 34 34 39 45 | 2c | 30 | 2c | 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 30 35 | 2c | 30 2e 35 35 33 37 34 38 | 2c |33 33 2e 37 00 //定位信息（0x00结尾字符串，表示如下：1.纬度,经度,高程,时间,速度,方向；2.分隔符为半角< 分隔符为0x2c >）

ba cd d0 cb c2 b7 00 //站台信息（0x00结尾字符串）

30 2e 35 35 33 37 34 38 00 //行驶速度（0x00结尾字符串）

00 //行驶方向

02 //客流负载

03 //运行状态

02 //与前车间距

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 0

95 98 03 98

29ce4 29cee\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*convert to 8005 end

len = 8

key is: 88 E5 FD F8 11 5D B4 F5 38 52 52 8D 6C DB 03 AD 51 6B 06 0F 14 78 22 83

before encrypt:

95 98 03 98 04 04 04 04

after encrypt :

00 00 00 00 41 81 F1 6C 29 26 5D B6

return as:

00 01 00 18 41 88 E5 FD F8 11 5D B4 F5 38 52 52 8D 6C DB 03 AD 51 6B 06 0F 14 78 22 83 81 F1 6C 29 26 5D B6

return len = 36:

convert\_string start

diff\_time=0.000007

prev\_time=-28488 this\_time=-28488

41 4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710449E,0,19-▒3-29 15:07:05,0.553748,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710449

gps\_info[0][0] = 100.000000

hight = 0

30

speed=5

gps\_info[1][0] = 0.000001

gps\_info[3][0] = 5.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 1.666667

33 33 direction=33

direction= 00 21

convert\_string end

29ce4 29cee\*\*\*\*\*\*\*\*\*\*\*covert recived uart to 8009

35 39 c2 b7 01 00 01 01 50 00 00 02 b9 0e 75 07 8d 72 b1 00 00 00 05 00 21 19 03 29 15 07 05 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 41 4c 30 30 30 35

len = 64

key is: 88 E5 FD F8 11 5D B4 F5 38 52 52 8D 6C DB 03 AD 51 6B 06 0F 14 78 22 83

before encrypt:

35 39 C2 B7 01 00 01 01 50 00 00 02 B9 0E 75 07 8D 72 B1 00 00 00 05 00 21 19 03 29 15 07 05 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 41 4C 30 30 30 35 01 04 04 04 04

after encrypt :

00 01 00 18 AB D4 19 4A 22 93 93 6C B1 DA 5F CF 65 E3 35 97 C8 BD A9 44 13 84 74 AF 72 B5 02 D9 86 34 B6 68 88 78 F0 F4 43 B8 7F 8E 88 78 F0 F4 43 B8 7F 8E DD 60 E9 5A 6D 34 B6 68 69 27 A8 F5 B7 16 D9 3A

return as:

00 19 00 18 AB D4 19 4A 22 93 93 6C B1 DA 5F CF 65 E3 35 97 C8 BD A9 44 13 84 74 AF 72 88 E5 FD F8 11 5D B4 F5 38 52 52 8D 6C DB 03 AD 51 6B 06 0F 14 78 22 83 B5 02 D9 86 34 B6 68 88 78 F0 F4 43 B8 7F 8E 88 78 F0 F4 43 B8 7F 8E DD 60 E9 5A 6D 34 B6 68 69 27 A8 F5 B7 16 D9 3A

return len = 92:

len = 40

key is: 88 E5 FD F8 11 5D B4 F5 38 52 52 8D 6C DB 03 AD 51 6B 06 0F 14 78 22 83

before encrypt:

00 00 00 00 02 41 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 03 03

after encrypt :

00 19 00 18 AB B5 11 38 E9 B5 75 07 88 78 F0 F4 43 B8 7F 8E 88 78 F0 F4 43 B8 7F 8E 88 78 F0 F4 43 B8 7F 8E 21 C0 3C 1B 03 D0 7D 94

return as:

00 01 00 18 AB 88 E5 FD F8 11 5D B4 F5 38 52 52 8D 6C DB 03 AD 51 6B 06 0F 14 78 22 83 B5 11 38 E9 B5 75 07 88 78 F0 F4 43 B8 7F 8E 88 78 F0 F4 43 B8 7F 8E 88 78 F0 F4 43 B8 7F 8E 21 C0 3C 1B 03 D0 7D 94

return len = 68:

29ce4 29cee \*\*\*\*\*\*\*\*\*covert recived uart to 8014

convert\_string start

diff\_time=0.037092

prev\_time=-28488 this\_time=-28488

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710449E,0,19-▒3-29 15:07:05,0.553748,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710449

gps\_info[0][0] = 100.000000

hight = 0

30

speed=5

gps\_info[1][0] = 0.005153

gps\_info[3][0] = 5.000000

gps\_info[4][0] = 5.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 3.333333

33 33 direction=33

direction= 00 21

convert\_string end

buffer\_send\_rsu\_len = 59

7e 80 05 08 24 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 02 00 01 00 18 41 88 e5 fd f8 11 5d b4 f5 38 52 52 8d 6c db 03 ad 51 6b 06 0f 14 78 22 83 81 f1 6c 29 26 5d b6 4a 7e

send nbytes = 59

\*发送给服务器的数据\*\*\*\*\*\*\*

buffer\_send\_rsu\_len = 115

7e 80 09 08 5c 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 03 00 19 00 18 ab d4 19 4a 22 93 93 6c b1 da 5f cf 65 e3 35 97 c8 bd a9 44 13 84 74 af 72 88 e5 fd f8 11 5d b4 f5 38 52 52 8d 6c db 03 ad 51 6b 06 0f 14 78 22 83 b5 02 d9 86 34 b6 68 88 78 f0 f4 43 b8 7f 8e 88 78 f0 f4 43 b8 7f 8e dd 60 e9 5a 6d 34 b6 68 69 27 a8 f5 b7 16 d9 3a 5f 7e

send nbytes = 115

\*发送给服务器的数据\*\*\*\*\*\*\*

buffer\_send\_rsu\_len = 92

7e 80 14 08 44 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 04 00 01 00 18 ab 88 e5 fd f8 11 5d b4 f5 38 52 52 8d 6c db 03 ad 51 6b 06 0f 14 78 22 83 b5 11 38 e9 b5 75 07 88 78 f0 f4 43 b8 7f 8e 88 78 f0 f4 43 b8 7f 8e 88 78 f0 f4 43 b8 7f 8e 21 c0 3c 1b 03 d0 7d 01 94 9f 7e

send nbytes = 92

\*发送给服务器的数据\*\*\*\*\*\*\*

save\_msg datalength = 10

ee 03 98 bb 03 98 ba 03 98 be 03 98 c0 03 98 bf

RSSI EE recived from uart

queueNo is 0

rssibuff[4][0]<5,dist by gps1=100

rssibuff[4][0]<5,dist by gps2=100

rssi=68.750000 dist=40 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 cf 00 75 00 00 40 19 03 29 15 07 06 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 34 39 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 30 36 2c 30 2e 31 36 32 39 37 36 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 31 36 32 39 37 36 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.966785

prev\_time=-28488 this\_time=-28487

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710449E,0,19-▒3-29 15:07:06,0.162976,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710449

gps\_info[0][0] = 100.000000

hight = 0

30

speed=1

gps\_info[1][0] = 0.032008

gps\_info[3][0] = 5.000000

gps\_info[4][0] = 5.000000

gps\_info[5][0] = 1.000000

gps\_info[6][0] = 3.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 b9 03 98 bb 03 98 bb 03 98 bc

RSSI EE recived from uart

queueNo is 0

rssi=66.333333 dist=37 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 b6 03 98 bd 03 98 bb 03 98 bd

RSSI EE recived from uart

queueNo is 0

rssi=69.333333 dist=41 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d1 00 75 00 00 40 19 03 29 15 07 10 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 31 30 2c 30 2e 37 36 38 35 38 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 37 36 38 35 38 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=3.759996

prev\_time=-28487 this\_time=-28483

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710464E,0,19-▒3-29 15:07:10,0.768580,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=7

gps\_info[1][0] = 0.763118

gps\_info[3][0] = 7.000000

gps\_info[4][0] = 5.000000

gps\_info[5][0] = 1.000000

gps\_info[6][0] = 4.333333

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d0 00 75 00 00 40 19 03 29 15 07 07 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 34 39 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 30 37 2c 30 2e 39 34 38 32 32 34 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 39 34 38 32 32 34 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=1.139931

prev\_time=-28483 this\_time=-28482

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710449E,0,19-▒3-29 15:07:07,0.948224,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710449

gps\_info[0][0] = 100.000000

hight = 0

30

speed=9

gps\_info[1][0] = 1.048101

gps\_info[3][0] = 7.000000

gps\_info[4][0] = 9.000000

gps\_info[5][0] = 1.000000

gps\_info[6][0] = 5.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b8 03 98 ba 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

rssi=67.666667 dist=39 return=99

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d2 00 75 00 00 40 19 03 29 15 07 12 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 31 32 2c 31 2e 31 33 38 39 38 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 31 33 38 39 38 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.890070

prev\_time=-28482 this\_time=-28481

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710464E,0,19-▒3-29 15:07:12,1.138980,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

31

speed=11

gps\_info[1][0] = 0.320067

gps\_info[3][0] = 7.000000

gps\_info[4][0] = 9.000000

gps\_info[5][0] = 11.000000

gps\_info[6][0] = 9.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b6 03 98 b8 03 98 bb 03 98 bc

RSSI EE recived from uart

queueNo is 0

rssi=72.500000 dist=45 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d3 00 75 00 00 40 19 03 29 15 07 13 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 31 33 2c 31 2e 37 32 32 33 36 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 37 32 32 33 36 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=1.200067

prev\_time=-28481 this\_time=-28480

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710464E,0,19-▒3-29 15:07:13,1.722360,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

31

speed=17

gps\_info[1][0] = 0.886765

gps\_info[3][0] = 17.000000

gps\_info[4][0] = 9.000000

gps\_info[5][0] = 11.000000

gps\_info[6][0] = 12.333333

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d4 00 75 00 00 40 19 03 29 15 07 14 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 31 34 2c 31 2e 31 33 38 39 38 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 31 33 38 39 38 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.799858

prev\_time=-28480 this\_time=-28479

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:07:14,1.138980,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

31

speed=11

gps\_info[1][0] = 1.131166

gps\_info[3][0] = 17.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 11.000000

gps\_info[6][0] = 13.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 bc 03 98 bc 03 98 bb

RSSI EE recived from uart

queueNo is 0

rssi=69.666667 dist=41 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 ba 03 98 ba 03 98 ba 03 98 b9 03 98 bb

save\_msg datalength = 10

ee 03 98 b9 03 98 ba 03 98 ba 03 98 ba 03 98 b9

RSSI EE recived from uart

queueNo is 0

rssi=68.333333 dist=40 return=101

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d7 00 75 00 00 40 19 03 29 15 07 17 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 31 37 2c 30 2e 32 36 38 35 34 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 32 36 38 35 34 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=4.111082

prev\_time=-28479 this\_time=-28475

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:07:17,0.268540,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=2

gps\_info[1][0] = 0.359560

gps\_info[3][0] = 17.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 2.000000

gps\_info[6][0] = 10.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b8 03 98 ba 03 98 ba 03 98 bb

RSSI EE recived from uart

queueNo is 0

rssi=70.250000 dist=42 return=101

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b9 03 98 ba 03 98 ba 03 98 b9 03 98 ba

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d6 00 75 00 00 40 19 03 29 15 07 16 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 31 36 2c 30 2e 31 32 35 39 33 36 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 31 32 35 39 33 36 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=1.589067

prev\_time=-28475 this\_time=-28474

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:07:16,0.125936,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=1

gps\_info[1][0] = 0.403700

gps\_info[3][0] = 1.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 2.000000

gps\_info[6][0] = 4.666667

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 d9 00 75 00 00 40 19 03 29 15 07 20 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 32 30 2c 31 2e 31 35 30 30 39 32 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 31 35 30 30 39 32 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.609918

prev\_time=-28474 this\_time=-28473

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:07:20,1.150092,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

31

speed=11

gps\_info[1][0] = 0.590064

gps\_info[3][0] = 1.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 2.000000

gps\_info[6][0] = 4.666667

33 33 direction=33

direction= 00 21

convert\_string end

xread n\_read = = 0save\_msg datalength = 0f

03 98 bb 03 98 bb 03 98 bb 03 98 bb 03 98 bb

save\_msg datalength = 10

ee 03 98 bb 03 98 b9 03 98 b9 03 98 ba 03 98 bb

RSSI EE recived from uart

queueNo is 0

rssi=69.500000 dist=41 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bb 03 98 bb 03 98 b9 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

rssi=70.000000 dist=42 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 ba 03 98 bb 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

rssi=71.000000 dist=43 return=100

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 db 00 75 00 00 40 19 03 29 15 07 23 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 32 33 2c 31 2e 34 37 34 31 39 32 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 34 37 34 31 39 32 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=2.399947

prev\_time=-28473 this\_time=-28471

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:07:23,1.474192,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

31

speed=14

gps\_info[1][0] = 1.523377

gps\_info[3][0] = 1.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 14.000000

gps\_info[6][0] = 8.666667

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 b9 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

rssi=69.000000 dist=40 return=99

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 dc 00 75 00 00 40 19 03 29 15 07 24 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 32 34 2c 32 2e 32 30 30 31 37 36 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 32 2e 32 30 30 31 37 36 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.929975

prev\_time=-28471 this\_time=-28470

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:07:24,2.200176,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

32

speed=22

gps\_info[1][0] = 1.091695

gps\_info[3][0] = 22.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 14.000000

gps\_info[6][0] = 15.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 dd 00 75 00 00 40 19 03 29 15 07 25 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 32 35 2c 31 2e 31 31 36 37 35 36 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 31 31 36 37 35 36 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=1.070067

prev\_time=-28470 this\_time=-28469

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:07:25,1.116756,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

31

speed=11

gps\_info[1][0] = 1.418660

gps\_info[3][0] = 22.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 14.000000

gps\_info[6][0] = 15.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 bc 03 98 bb 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

rssi=70.666667 dist=42 return=99

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 de 00 75 00 00 40 19 03 29 15 07 25 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 32 35 2c 32 2e 35 31 31 33 31 32 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 32 2e 35 31 31 33 31 32 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.599899

prev\_time=-28469 this\_time=-28468

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:07:25,2.511312,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

32

speed=25

gps\_info[1][0] = 0.835256

gps\_info[3][0] = 22.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 25.000000

gps\_info[6][0] = 19.333333

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 35 df 00 75 00 00 40 19 03 29 15 07 26 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 34 39 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 37 3a 32 36 2c 31 2e 37 36 33 31 30 34 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 37 36 33 31 30 34 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.699962

prev\_time=-28468 this\_time=-28467

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710449E,0,19-▒3-29 15:07:26,1.763104,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710449

gps\_info[0][0] = 98.000000

hight = 0

31

speed=17

gps\_info[1][0] = 1.165794

gps\_info[3][0] = 17.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 25.000000

gps\_info[6][0] = 17.666667

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b6 03 98 b8 03 98 ba 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

rssi=68.750000 dist=40 return=97

flag = 02,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

[1] + Stopped ./taxier

~ $ ./kill.sh

[1] + Killed ./taxier

~ $ ./kill.sh

killall: watch2.sh: no process killed

killall: watch3.sh: no process killed

killall: taxier: no process killed

~ $ ./kill.sh

killall: watch2.sh: no process killed

killall: watch3.sh: no process killed

killall: taxier: no process killed

~ $ ./taxier

value\_access = 0

打开数据库

portnum = 65001

ipadd = 47.94.44.231

device\_id is = 01016000 device\_id\_hex is = 30

device\_id\_hex is = 31

device\_id\_hex is = 30

device\_id\_hex is = 31

device\_id\_hex is = 36

device\_id\_hex is = 30

device\_id\_hex is = 30

device\_id\_hex is = 30

station\_id is = 01015000

station\_id is = 01

station\_id is = 01

station\_id is = 50

station\_id is = 00

DEBUG = 1

CRYPT= 1

floor\_value = 0

WEIDU = 45681641

JINGDU = 126709557

funa = 62.050000

funb = 1.190000

func = 115.000000

HEARTBEAT = 30

RADAR\_PARAMENT = 101

open /dev/ttyAMA1

open\_uart success

init is OK

end of openfile

enter save\_msg\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

enter send\_msg \*\*\*\*\*\*\*\*\*\*\*

enter rec\_ask \*\*\*\*\*\*\*\*\*\*\*

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 bb 03 98 bb 03 98 b8

RSSI EE recived from uart

queueNo is -1

queueno=-1 new id : 03 98

queueNo=-1 rssi=70.000000 dist=24 return=24

queueNo=-1,03,98

queueNo=-1 8=03,9=03

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b9 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps6=0

rssi=69.333333 dist=41 return=0

flag = 05,

8=03,9=01

7e 0b ee 00 03 98 00 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 06 00 75 00 00 40 19 03 29 15 08 44 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 36 36 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 34 34 2c 31 2e 31 37 34 31 36 38 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 31 37 34 31 36 38 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 0

95 98 03 98

29ce4 29cee\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*convert to 8005 end

len = 8

key is: F2 42 3E 7B F7 56 34 53 B2 59 80 8F 4C CF DB 68 8D 24 21 FE 9E 6B 54 A7

before encrypt:

95 98 03 98 04 04 04 04

after encrypt :

00 00 00 00 C7 12 3A 01 EE 61 C7 BB

return as:

00 07 00 18 C7 12 3A 01 EE 61 C7 F2 42 3E 7B F7 56 34 53 B2 59 80 8F 4C CF DB 68 8D 24 21 FE 9E 6B 54 A7 BB

return len = 36:

convert\_string start

diff\_time=0.000006

prev\_time=-28389 this\_time=-28389

41 4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710464E,0,19-▒3-29 15:08:44,1.174168,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710464

gps\_info[0][0] = 98.000000

hight = 0

31

speed=11

gps\_info[1][0] = 0.000002

gps\_info[3][0] = 11.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 3.666667

33 33 direction=33

direction= 00 21

convert\_string end

29ce4 29cee\*\*\*\*\*\*\*\*\*\*\*covert recived uart to 8009

35 39 c2 b7 01 00 01 01 50 00 00 02 b9 0e 5a 07 8d 72 c0 00 00 00 0b 00 21 19 03 29 15 08 44 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 41 4c 30 30 30 35

len = 64

key is: F2 42 3E 7B F7 56 34 53 B2 59 80 8F 4C CF DB 68 8D 24 21 FE 9E 6B 54 A7

before encrypt:

35 39 C2 B7 01 00 01 01 50 00 00 02 B9 0E 5A 07 8D 72 C0 00 00 00 0B 00 21 19 03 29 15 08 44 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 41 4C 30 30 30 35 01 04 04 04 04

after encrypt :

00 07 00 18 1D 24 6F 13 92 F2 94 63 A0 2D 22 E0 D8 41 BE 55 CA 99 BC 81 3F B2 0E 52 29 5A 02 EF 4A 58 52 6E 26 21 A0 F6 A4 46 A6 C7 26 21 A0 F6 A4 46 A6 C7 8E E2 12 95 28 C1 28 A8 BA 4C 08 70 81 9D DB E2

return as:

00 1F 00 18 1D 24 6F 13 92 F2 94 63 A0 2D 22 E0 D8 41 BE 55 CA 99 BC 81 3F B2 0E 52 29 5A 02 EF 4A 58 52 F2 42 3E 7B F7 56 34 53 B2 59 80 8F 4C CF DB 68 8D 24 21 FE 9E 6B 54 A7 6E 26 21 A0 F6 A4 46 A6 C7 26 21 A0 F6 A4 46 A6 C7 8E E2 12 95 28 C1 28 A8 BA 4C 08 70 81 9D DB E2

return len = 92:

len = 40

key is: F2 42 3E 7B F7 56 34 53 B2 59 80 8F 4C CF DB 68 8D 24 21 FE 9E 6B 54 A7

before encrypt:

00 00 00 00 02 41 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 03 03 03

after encrypt :

00 1F 00 18 82 3C EB 36 A5 EB 70 1A 26 21 A0 F6 A4 46 A6 C7 26 21 A0 F6 A4 46 A6 C7 26 21 A0 F6 A4 46 A6 C7 4E B5 8E 93 15 5A 21 6E

return as:

00 1F 00 18 82 3C EB 36 A5 EB 70 1A 26 21 A0 F6 A4 46 A6 C7 26 21 A0 F6 A4 46 A6 C7 26 21 A0 F6 A4 46 A6 F2 42 3E 7B F7 56 34 53 B2 59 80 8F 4C CF DB 68 8D 24 21 FE 9E 6B 54 A7 C7 4E B5 8E 93 15 5A 21 6E

return len = 68:

29ce4 29cee \*\*\*\*\*\*\*\*\*covert recived uart to 8014

convert\_string start

diff\_time=0.289964

prev\_time=-28389 this\_time=-28388

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710464E,0,19-▒3-29 15:08:44,1.174168,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710464

gps\_info[0][0] = 98.000000

hight = 0

31

speed=11

gps\_info[1][0] = 0.088602

gps\_info[3][0] = 11.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 7.333333

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

in newdist gps\_info[1][0] = 0

rssi=69.750000 dist=41 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

buffer\_send\_rsu\_len = 59

7e 80 05 08 24 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 01 00 07 00 18 c7 12 3a 01 ee 61 c7 f2 42 3e 7b f7 56 34 53 b2 59 80 8f 4c cf db 68 8d 24 21 fe 9e 6b 54 a7 bb 4b 7e

send nbytes = 59

\*发送给服务器的数据\*\*\*\*\*\*\*

buffer\_send\_rsu\_len = 115

7e 80 09 08 5c 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 02 00 1f 00 18 1d 24 6f 13 92 f2 94 63 a0 2d 22 e0 d8 41 be 55 ca 99 bc 81 3f b2 0e 52 29 5a 02 ef 4a 58 52 f2 42 3e 7b f7 56 34 53 b2 59 80 8f 4c cf db 68 8d 24 21 fe 9e 6b 54 a7 6e 26 21 a0 f6 a4 46 a6 c7 26 21 a0 f6 a4 46 a6 c7 8e e2 12 95 28 c1 28 a8 ba 4c 08 70 81 9d db e2 f0 7e

send nbytes = 115

\*发送给服务器的数据\*\*\*\*\*\*\*

buffer\_send\_rsu\_len = 91

7e 80 14 08 44 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 03 00 1f 00 18 82 3c eb 36 a5 eb 70 1a 26 21 a0 f6 a4 46 a6 c7 26 21 a0 f6 a4 46 a6 c7 26 21 a0 f6 a4 46 a6 f2 42 3e 7b f7 56 34 53 b2 59 80 8f 4c cf db 68 8d 24 21 fe 9e 6b 54 a7 c7 4e b5 8e 93 15 5a 21 6e 4e 7e

send nbytes = 91

\*发送给服务器的数据\*\*\*\*\*\*\*

save\_msg datalength = 10

ee 03 98 bb 03 98 bb 03 98 bc 03 98 bb 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=98

rssi=69.000000 dist=40 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 07 00 75 00 00 40 19 03 29 15 08 45 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 36 36 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 34 35 2c 33 2e 31 39 30 39 39 36 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 33 2e 31 39 30 39 39 36 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 1

convert\_string start

diff\_time=0.605443

prev\_time=-28388 this\_time=-28388

41 4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710464E,0,19-▒3-29 15:08:45,3.190996,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710464

gps\_info[0][0] = 98.000000

hight = 0

33

speed=31

gps\_info[1][0] = 0.521354

gps\_info[3][0] = 11.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 31.000000

gps\_info[6][0] = 17.666667

33 33 direction=33

direction= 00 21

convert\_string end

\*\*\*\*\*\*\*\*\*\*\*\*\*\*发生滞后线\*\*\*\*\*\*\*\*\*\*\*\*\*

29ce4 29cee \*\*\*\*\*\*\*\*\*\*\*\*\*\*covert recived uart to 8011

35 39 c2 b7 00 00 01 01 50 00 01 00 02 b9 0e 5a 07 8d 72 c0 00 00 00 1f 00 21 19 03 29 15 08 45 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 04 00 01 00 00 00 00 00 00 00 03 41 4c 30 30 30 35 01

len = 72

key is: E7 D1 56 1C 03 61 0A 28 E1 8A 91 49 DE E7 15 29 26 87 13 94 CA 8A D4 79

before encrypt:

35 39 C2 B7 00 00 01 01 50 00 01 00 02 B9 0E 5A 07 8D 72 C0 00 00 00 1F 00 21 19 03 29 15 08 45 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 04 00 01 00 00 00 00 00 00 00 03 41 4C 30 30 30 35 01 05 05 05 05 05

after encrypt :

00 1F 00 18 09 F1 35 0C C2 0E 2A 9C DC 32 CB FF D2 5D 8F A8 C8 A1 5D EE B3 24 5B D1 F5 5E 83 E0 86 47 BC 76 00 00 69 6A 7B 62 36 7D 00 00 69 6A 7B 62 36 7D AC CA 46 5B 52 9D E0 0E C8 4D ED 82 C1 32 2E E6 33 65 34 2A BA 96 B8 29

return as:

00 3F 00 18 09 F1 35 0C C2 0E 2A 9C DC 32 CB FF D2 5D 8F A8 C8 A1 5D EE B3 24 5B D1 F5 5E 83 E0 86 47 BC 76 00 00 69 6A 7B 62 36 7D 00 00 69 6A 7B 62 36 7D AC CA 46 5B 52 9D E0 0E C8 4D ED 82 C1 32 2E E7 D1 56 1C 03 61 0A 28 E1 8A 91 49 DE E7 15 29 26 87 13 94 CA 8A D4 79 E6 33 65 34 2A BA 96 B8 29

return len = 100:

convert\_string start

diff\_time=0.026892

prev\_time=-28388 this\_time=-28388

41 4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710464E,0,19-▒3-29 15:08:45,3.190996,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710464

gps\_info[0][0] = 98.000000

hight = 0

33

speed=31

gps\_info[1][0] = 0.544511

gps\_info[3][0] = 31.000000

gps\_info[4][0] = 11.000000

gps\_info[5][0] = 31.000000

gps\_info[6][0] = 24.333333

33 33 direction=33

direction= 00 21

convert\_string end

29ce4 29cee \*\*\*\*\*\*\*\*\*\*covert recived uart to 8013

35 39 c2 b7 00 00 02 b9 0e 5a 07 8d 72 c0 00 00 00 1f 00 21 19 03 29 15 08 45 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 01 00 00 00 00 01 01 50 00 00 00 00 00 00

len = 56

key is: E7 D1 56 1C 03 61 0A 28 E1 8A 91 49 DE E7 15 29 26 87 13 94 CA 8A D4 79

before encrypt:

35 39 C2 B7 00 00 02 B9 0E 5A 07 8D 72 C0 00 00 00 1F 00 21 19 03 29 15 08 45 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 01 00 00 00 07 07 07 07 07 07 07

after encrypt :

00 3F 00 18 FB AC 8D DC FB 02 F9 A4 4A BB D2 39 33 CD F6 E1 D0 EC D2 9B 9E 8B 77 EE 63 D9 53 11 2E F0 71 A2 00 00 69 6A 7B 62 36 7D EA 5A 24 12 2F 64 C2 70 E4 B6 78 86 46 40 78 02

return as:

00 0F 00 18 FB AC 8D DC FB 02 F9 A4 4A BB D2 39 33 CD F6 E7 D1 56 1C 03 61 0A 28 E1 8A 91 49 DE E7 15 29 26 87 13 94 CA 8A D4 79 E1 D0 EC D2 9B 9E 8B 77 EE 63 D9 53 11 2E F0 71 A2 00 00 69 6A 7B 62 36 7D EA 5A 24 12 2F 64 C2 70 E4 B6 78 86 46 40 78 02

return len = 84:

convert\_string start

diff\_time=0.024525

prev\_time=-28388 this\_time=-28388

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710464E,0,19-▒3-29 15:08:45,3.190996,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710464

gps\_info[0][0] = 98.000000

hight = 0

33

speed=31

gps\_info[1][0] = 0.565629

gps\_info[3][0] = 31.000000

gps\_info[4][0] = 31.000000

gps\_info[5][0] = 31.000000

gps\_info[6][0] = 31.000000

33 33 direction=33

direction= 00 21

convert\_string end

buffer\_send\_rsu\_len = 125

7e 80 11 08 64 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 05 00 3f 00 18 09 f1 35 0c c2 0e 2a 9c dc 32 cb ff d2 5d 8f a8 c8 a1 5d ee b3 24 5b d1 f5 5e 83 e0 86 47 bc 76 00 00 69 6a 7b 62 36 7d 01 00 00 69 6a 7b 62 36 7d 01 ac ca 46 5b 52 9d e0 0e c8 4d ed 82 c1 32 2e e7 d1 56 1c 03 61 0a 28 e1 8a 91 49 de e7 15 29 26 87 13 94 ca 8a d4 79 e6 33 65 34 2a ba 96 b8 29 5b 7e

send nbytes = 125

\*发送给服务器的数据\*\*\*\*\*\*\*

buffer\_send\_rsu\_len = 108

7e 80 13 08 54 01 34 39 38 25 61 30 31 30 31 36 30 30 30 00 05 00 0f 00 18 fb ac 8d dc fb 02 f9 a4 4a bb d2 39 33 cd f6 e7 d1 56 1c 03 61 0a 28 e1 8a 91 49 de e7 15 29 26 87 13 94 ca 8a d4 79 e1 d0 ec d2 9b 9e 8b 77 ee 63 d9 53 11 2e f0 save\_msg datalength = 10

ee 03 98 bb 03 98 bb 03 98 bb 03 98 bc 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=98

rssi=69.000000 dist=40 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

71 a2 00 00 69 6a 7b 62 36 7d 01 ea 5a 24 12 2f 64 c2 70 e4 b6 78 86 46 40 78 02 49 7e

send nbytes = 108

\*发送给服务器的数据\*\*\*\*\*\*\*

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 bb 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=98

rssi=69.000000 dist=40 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 08 00 75 00 00 40 19 03 29 15 08 46 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 34 36 2c 31 2e 36 34 32 37 32 34 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 36 34 32 37 32 34 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.947180

prev\_time=-28388 this\_time=-28387

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:08:46,1.642724,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

31

speed=16

gps\_info[1][0] = 0.986598

gps\_info[3][0] = 31.000000

gps\_info[4][0] = 31.000000

gps\_info[5][0] = 16.000000

gps\_info[6][0] = 26.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 ba 03 98 b8 03 98 b9 03 98 bc 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=70.000000 dist=42 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 bc 03 98 bc 03 98 bc 03 98 b9 03 98 b9

save\_msg datalength = 10

ee 03 98 b7 03 98 b9 03 98 b8 03 98 ba 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.500000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 09 00 75 00 00 40 19 03 29 15 08 48 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 34 38 2c 30 2e 38 31 33 30 32 38 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 38 31 33 30 32 38 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.799951

prev\_time=-28387 this\_time=-28385

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:08:48,0.813028,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=8

gps\_info[1][0] = 1.386587

gps\_info[3][0] = 8.000000

gps\_info[4][0] = 31.000000

gps\_info[5][0] = 16.000000

gps\_info[6][0] = 18.333333

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 bb 03 98 ba 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=70.000000 dist=42 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 ba 03 98 bb 03 98 bc 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=69.000000 dist=40 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 bd 03 98 bc 03 98 bd 03 98 bd 03 98 bb

save\_msg datalength = 10

ee 03 98 ba 03 98 bb 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=67.750000 dist=39 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bb 03 98 bc 03 98 be 03 98 be 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=67.000000 dist=38 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bc 03 98 bd 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=67.000000 dist=38 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 0b 00 75 00 00 40 19 03 29 15 08 51 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 31 2c 30 2e 32 32 32 32 34 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 32 32 32 32 34 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.710000

prev\_time=-28385 this\_time=-28382

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:08:51,0.222240,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=2

gps\_info[1][0] = 1.537143

gps\_info[3][0] = 8.000000

gps\_info[4][0] = 2.000000

gps\_info[5][0] = 16.000000

gps\_info[6][0] = 8.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 bc 03 98 bd 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=67.000000 dist=38 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 0c 00 75 00 00 40 19 03 29 15 08 52 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 32 2c 30 2e 36 31 33 30 31 32 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 36 31 33 30 31 32 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.789997

prev\_time=-28382 this\_time=-28381

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:08:52,0.613012,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=6

gps\_info[1][0] = 1.668809

gps\_info[3][0] = 8.000000

gps\_info[4][0] = 2.000000

gps\_info[5][0] = 6.000000

gps\_info[6][0] = 5.333333

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 be 03 98 bd 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=66.500000 dist=37 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 be 03 98 be 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=66.000000 dist=37 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 0d 00 75 00 00 40 19 03 29 15 08 52 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 32 2c 30 2e 37 37 39 36 39 32 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 37 37 39 36 39 32 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800021

prev\_time=-28381 this\_time=-28381

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:08:52,0.779692,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=7

gps\_info[1][0] = 1.824369

gps\_info[3][0] = 7.000000

gps\_info[4][0] = 2.000000

gps\_info[5][0] = 6.000000

gps\_info[6][0] = 5.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 bd 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=66.000000 dist=37 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 be 03 98 be 03 98 be 03 98 bd 03 98 bd

save\_msg datalength = 10

ee 03 98 bb 03 98 ba 03 98 b9 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=66.500000 dist=37 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 0f 00 75 00 00 40 19 03 29 15 08 54 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 34 2c 31 2e 39 33 37 31 39 32 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 31 2e 39 33 37 31 39 32 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.899950

prev\_time=-28381 this\_time=-28379

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:08:54,1.937192,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

31

speed=19

gps\_info[1][0] = 2.827120

gps\_info[3][0] = 7.000000

gps\_info[4][0] = 19.000000

gps\_info[5][0] = 6.000000

gps\_info[6][0] = 10.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b9 03 98 b9 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.500000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 ba 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.500000 dist=42 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bb 03 98 bb 03 98 bb 03 98 bb 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.000000 dist=42 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 10 00 75 00 00 40 19 03 29 15 08 55 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 35 2c 30 2e 35 34 36 33 34 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 35 34 36 33 34 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.099966

prev\_time=-28379 this\_time=-28378

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:08:55,0.546340,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=5

gps\_info[1][0] = 2.979893

gps\_info[3][0] = 7.000000

gps\_info[4][0] = 19.000000

gps\_info[5][0] = 5.000000

gps\_info[6][0] = 10.333333

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 bc 03 98 be 03 98 bf 03 98 bf

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=68.750000 dist=40 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 bc 03 98 be 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=65.500000 dist=36 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 11 00 75 00 00 40 19 03 29 15 08 57 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 36 36 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 37 2c 30 2e 35 31 36 37 30 38 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 35 31 36 37 30 38 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.210091

prev\_time=-28378 this\_time=-28376

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710480E,0,19-▒3-29 15:08:57,0.516708,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710480

gps\_info[0][0] = 99.000000

hight = 0

30

speed=5

gps\_info[1][0] = 3.147961

gps\_info[3][0] = 5.000000

gps\_info[4][0] = 19.000000

gps\_info[5][0] = 5.000000

gps\_info[6][0] = 9.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=68.000000 dist=39 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 be 03 98 be 03 98 bf

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=67.000000 dist=38 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 76

09 32 95 98 00 03 98 d0 c1 36 12 00 75 00 00 40 19 03 29 15 08 58 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 36 36 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 82 33 2d 32 39 20 31 35 3a 30 38 3a 35 38 2c 30 2e 37 34 30 38 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 37 34 30 38 30 30 00 00 02 03 02 03

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.009903

prev\_time=-28376 this\_time=-28375

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710480E,0,19-▒3-29 15:08:58,0.740800,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710480

gps\_info[0][0] = 99.000000

hight = 0

30

speed=7

gps\_info[1][0] = 3.344331

gps\_info[3][0] = 5.000000

gps\_info[4][0] = 7.000000

gps\_info[5][0] = 5.000000

gps\_info[6][0] = 5.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bf 03 98 be 03 98 be 03 98 be 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=65.500000 dist=36 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 be 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=66.000000 dist=37 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 13 00 75 00 00 40 19 03 29 15 08 58 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 36 36 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 38 2c 30 2e 37 35 39 33 32 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 37 35 39 33 32 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.799921

prev\_time=-28375 this\_time=-28375

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710480E,0,19-▒3-29 15:08:58,0.759320,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710480

gps\_info[0][0] = 99.000000

hight = 0

30

speed=7

gps\_info[1][0] = 3.499872

gps\_info[3][0] = 5.000000

gps\_info[4][0] = 7.000000

gps\_info[5][0] = 7.000000

gps\_info[6][0] = 6.333333

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 be 03 98 be 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=67.000000 dist=38 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 be 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=66.000000 dist=37 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 14 00 75 00 00 40 19 03 29 15 08 59 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 36 36 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 38 3a 35 39 2c 30 2e 34 38 31 35 32 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 34 38 31 35 32 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.902961

prev\_time=-28375 this\_time=-28374

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710464E,0,19-▒3-29 15:08:59,0.481520,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710464

gps\_info[0][0] = 98.000000

hight = 0

30

speed=4

gps\_info[1][0] = 3.600201

gps\_info[3][0] = 4.000000

gps\_info[4][0] = 7.000000

gps\_info[5][0] = 7.000000

gps\_info[6][0] = 6.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 be 03 98 bf 03 98 bf 03 98 c0 03 98 c0

RSSI EE recived from uart

queueNo is 0

dist by gps7=98

rssi=66.000000 dist=37 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 15 00 75 00 00 40 19 03 29 15 09 00 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 36 36 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 30 2c 30 2e 33 35 35 35 38 34 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 33 35 35 35 38 34 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.697124

prev\_time=-28374 this\_time=-28373

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682266N,126.710464E,0,19-▒3-29 15:09:00,0.355584,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682266

jingdu = 126710464

gps\_info[0][0] = 98.000000

hight = 0

30

speed=3

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 4.000000

gps\_info[4][0] = 3.000000

gps\_info[5][0] = 7.000000

gps\_info[6][0] = 4.666667

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 c0 03 98 c0 03 98 c0 03 98 bf 03 98 bf

RSSI EE recived from uart

queueNo is 0

dist by gps7=98

rssi=64.000000 dist=34 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 bf 03 98 be 03 98 bf

RSSI EE recived from uart

queueNo is 0

dist by gps7=98

rssi=64.500000 dist=35 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 be 03 98 bc 03 98 bc 03 98 bc 03 98 bd

save\_msg datalength = 10

ee 03 98 bd 03 98 be 03 98 be 03 98 bd 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=98

rssi=65.500000 dist=36 return=98

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 62 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 17 00 75 00 00 40 19 03 29 15 09 02 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.000013

prev\_time=-28373 this\_time=-28371

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:02,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 4.000000

gps\_info[4][0] = 3.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 2.333333

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 bb 03 98 bb 03 98 bb 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=66.333333 dist=37 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 18 00 75 00 00 40 19 03 29 15 09 03 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800048

prev\_time=-28371 this\_time=-28370

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:03,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 3.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 1.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 bc 03 98 bb 03 98 bc 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=69.000000 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bc 03 98 bd 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 19 00 75 00 00 40 19 03 29 15 09 04 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.909970

prev\_time=-28370 this\_time=-28369

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:04,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=67.000000 dist=38 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bd 03 98 bc 03 98 bc 03 98 bc 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=67.000000 dist=38 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 1a 00 75 00 00 40 19 03 29 15 09 05 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.690115

prev\_time=-28369 this\_time=-28369

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:05,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bc 03 98 bc 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bc 03 98 bc 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 1b 00 75 00 00 40 19 03 29 15 09 06 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 36 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.999927

prev\_time=-28369 this\_time=-28368

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:06,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bc 03 98 bc 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=67.000000 dist=38 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 1c 00 75 00 00 40 19 03 29 15 09 07 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.310007

prev\_time=-28368 this\_time=-28366

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:07,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 bc 03 98 bb 03 98 bb 03 98 bb 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 1d 00 75 00 00 40 19 03 29 15 09 08 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.690089

prev\_time=-28366 this\_time=-28366

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:08,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bc 03 98 bc 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=69.000000 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bc 03 98 bd 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 1e 00 75 00 00 40 19 03 29 15 09 09 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 30 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.999935

prev\_time=-28366 this\_time=-28365

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:09:09,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 be 03 98 be 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=67.000000 dist=38 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 be 03 98 be 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=66.000000 dist=37 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 1f 00 75 00 00 40 19 03 29 15 09 10 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 31 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.109977

prev\_time=-28365 this\_time=-28364

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:09:10,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 bd 03 98 be 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=66.000000 dist=37 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 bd 03 98 be 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=67.000000 dist=38 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 20 00 75 00 00 40 19 03 29 15 09 11 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 31 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.000085

prev\_time=-28364 this\_time=-28363

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:11,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 be 03 98 be 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=67.000000 dist=38 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bd 03 98 be 03 98 be 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=66.000000 dist=37 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bd 03 98 bc 03 98 bc 03 98 bc 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=66.000000 dist=37 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 21 00 75 00 00 40 19 03 29 15 09 12 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 31 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.089829

prev\_time=-28363 this\_time=-28361

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:12,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bc 03 98 bd 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 22 00 75 00 00 40 19 03 29 15 09 13 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 31 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.099967

prev\_time=-28361 this\_time=-28360

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:13,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 bd 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 be 03 98 bd 03 98 be 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=67.000000 dist=38 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 23 00 75 00 00 40 19 03 29 15 09 14 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 31 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.810050

prev\_time=-28360 this\_time=-28360

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:14,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 bc 03 98 bc 03 98 bc 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=66.000000 dist=37 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 24 00 75 00 00 40 19 03 29 15 09 14 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 31 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.701542

prev\_time=-28360 this\_time=-28359

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:14,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 b9 03 98 ba 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.000000 dist=39 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bc 03 98 bc 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=69.333333 dist=41 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 bb 03 98 bb 03 98 bb 03 98 bb 03 98 bb

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 bb 03 98 ba 03 98 bb 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.250000 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bb 03 98 bb 03 98 bb 03 98 ba 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=69.000000 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 26 00 75 00 00 40 19 03 29 15 09 17 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 31 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.298424

prev\_time=-28359 this\_time=-28357

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:17,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 ba 03 98 b9 03 98 b8 03 98 b8 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.000000 dist=42 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b9 03 98 b9 03 98 b7 03 98 b7 03 98 b8

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 bb 03 98 ba 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.500000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 28 00 75 00 00 40 19 03 29 15 09 20 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 32 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=3.120044

prev\_time=-28357 this\_time=-28353

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:09:20,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 be 03 98 bd 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=69.000000 dist=40 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 be 03 98 be 03 98 be

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=66.000000 dist=37 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 be 03 98 be 03 98 be 03 98 bd 03 98 bd

save\_msg datalength = 10

ee 03 98 bd 03 98 bd 03 98 bd 03 98 bd 03 98 bd

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=66.000000 dist=37 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 2a 00 75 00 00 40 19 03 29 15 09 22 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 32 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.800063

prev\_time=-28353 this\_time=-28352

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:09:22,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bd 03 98 be 03 98 be 03 98 bf 03 98 bf

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=67.000000 dist=38 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 2b 00 75 00 00 40 19 03 29 15 09 22 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 32 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.889954

prev\_time=-28352 this\_time=-28351

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:09:22,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 be 03 98 be 03 98 bc 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=66.000000 dist=37 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 ba 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=68.666667 dist=40 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 2c 00 75 00 00 40 19 03 29 15 09 23 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 32 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.210113

prev\_time=-28351 this\_time=-28350

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:09:23,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 bc 03 98 bb 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=70.250000 dist=42 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b6 03 98 ba 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=70.666667 dist=42 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 ba 03 98 b9 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.333333 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b9 03 98 b5 03 98 b9 03 98 ba 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.500000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 b9 03 98 b7 03 98 b8 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=70.250000 dist=42 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 2e 00 75 00 00 40 19 03 29 15 09 28 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 32 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=8.000071

prev\_time=-28350 this\_time=-28342

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:28,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 b9 03 98 b8 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.333333 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.000000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 30 00 75 00 00 40 19 03 29 15 09 34 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 33 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.129872

prev\_time=-28342 this\_time=-28339

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:34,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 ba 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.000000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b9 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.500000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 31 00 75 00 00 40 19 03 29 15 09 35 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 33 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.999968

prev\_time=-28339 this\_time=-28338

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:35,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 2d 00 75 00 00 40 19 03 29 15 09 27 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 39 33 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 32 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.300087

prev\_time=-28338 this\_time=-28338

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682293N,126.710480E,0,19-▒3-29 15:09:27,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682293

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b9 03 98 b7 03 98 b9 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.500000 dist=45 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b9 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.000000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 bb 03 98 b8 03 98 b8 03 98 b6 03 98 b6

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b9 03 98 b6 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 ba 03 98 b7 03 98 b6 03 98 ba 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.333333 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 ba 03 98 b9 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.333333 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 33 00 75 00 00 40 19 03 29 15 09 39 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 33 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=4.079869

prev\_time=-28338 this\_time=-28334

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:39,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b9 03 98 b8 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.250000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.000000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 32 00 75 00 00 40 19 03 29 15 09 36 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 33 36 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.099982

prev\_time=-28334 this\_time=-28333

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:36,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b7 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.000000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 34 00 75 00 00 40 19 03 29 15 09 41 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 34 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800106

prev\_time=-28333 this\_time=-28332

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:41,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 ba 03 98 b7 03 98 b9 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.500000 dist=45 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b8 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.750000 dist=45 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 35 00 75 00 00 40 19 03 29 15 09 42 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 34 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.899896

prev\_time=-28332 this\_time=-28331

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:42,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b9 03 98 ba 03 98 b9 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.000000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 36 00 75 00 00 40 19 03 29 15 09 43 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 34 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.802747

prev\_time=-28331 this\_time=-28330

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:43,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b8 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.666667 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 37 00 75 00 00 40 19 03 29 15 09 43 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 34 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.597244

prev\_time=-28330 this\_time=-28330

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:43,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b8 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.000000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b7 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.000000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 38 00 75 00 00 40 19 03 29 15 09 45 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 34 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.110008

prev\_time=-28330 this\_time=-28329

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710464E,0,19-▒3-29 15:09:45,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710464

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b7 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.000000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.000000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b9 03 98 b7 03 98 b8 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.000000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 b8 03 98 b8 03 98 b8 03 98 b8 03 98 b8

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.500000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b9 03 98 b8 03 98 b9 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.000000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b8 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.250000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 3a 00 75 00 00 40 19 03 29 15 09 48 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 34 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=3.290080

prev\_time=-28329 this\_time=-28325

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:48,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b8 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 3b 00 75 00 00 40 19 03 29 15 09 49 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 34 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.019981

prev\_time=-28325 this\_time=-28324

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:49,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b8 03 98 b6 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b6 03 98 b8 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.500000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 3c 00 75 00 00 40 19 03 29 15 09 50 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.899996

prev\_time=-28324 this\_time=-28323

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:50,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b8 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b9 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=73.000000 dist=45 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 3d 00 75 00 00 40 19 03 29 15 09 51 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.000146

prev\_time=-28323 this\_time=-28322

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:51,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.750000 dist=45 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 3e 00 75 00 00 40 19 03 29 15 09 52 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.099892

prev\_time=-28322 this\_time=-28321

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:52,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b9 03 98 b8 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=73.000000 dist=45 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 3f 00 75 00 00 40 19 03 29 15 09 52 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.600068

prev\_time=-28321 this\_time=-28321

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:52,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b9 03 98 b9 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.500000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b7 03 98 b5 03 98 b6 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.000000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 40 00 75 00 00 40 19 03 29 15 09 53 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.789983

prev\_time=-28321 this\_time=-28320

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:53,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b8 03 98 b7 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=73.250000 dist=46 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b9 03 98 b9 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.500000 dist=45 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b8 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=73.000000 dist=45 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b8 03 98 b9 03 98 b8 03 98 b8 03 98 b7

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 42 00 75 00 00 40 19 03 29 15 09 57 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=3.599929

prev\_time=-28320 this\_time=-28316

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:57,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b6 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 bb 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=73.250000 dist=46 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 44 00 75 00 00 40 19 03 29 15 09 59 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.829924

prev\_time=-28316 this\_time=-28315

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:59,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 ba 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 ba 03 98 b9 03 98 b8 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 45 00 75 00 00 40 19 03 29 15 10 00 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 30 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.900082

prev\_time=-28315 this\_time=-28314

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:10:00,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b6 03 98 b7 03 98 b9 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.500000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b9 03 98 b9 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=72.000000 dist=44 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 46 00 75 00 00 40 19 03 29 15 10 00 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 30 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.099883

prev\_time=-28314 this\_time=-28313

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:00,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 ba 03 98 b9 03 98 b8 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.000000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b4 03 98 b6 03 98 b8 03 98 b9 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.333333 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 48 00 75 00 00 40 19 03 29 15 10 03 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 30 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.120045

prev\_time=-28313 this\_time=-28310

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:03,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 ba 03 98 ba 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.666667 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b7 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.500000 dist=42 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 bc 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.500000 dist=45 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 ba 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.000000 dist=42 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 4a 00 75 00 00 40 19 03 29 15 10 06 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 7e 78 09 32 95 98 00 03 98 d0 c1 36 47 00 75 00 00 40 19 03 29 15 10 01 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.882867

prev\_time=-28310 this\_time=-28308

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E~x 2▒▒locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = -593659022

speed=-48

direction=0

direction= 00 00

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 47 00 75 00 00 40 19 03 29 15 10 01 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 30 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.017295

prev\_time=-28308 this\_time=-28308

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:01,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b9 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.000000 dist=42 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b5 03 98 b4 03 98 b5 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.250000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 43 00 75 00 00 40 19 03 29 15 09 58 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 30 39 3a 35 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.169823

prev\_time=-28308 this\_time=-28306

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:09:58,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 b9 03 98 b9 03 98 b9 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=74.250000 dist=47 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 4b 00 75 00 00 40 19 03 29 15 10 07 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 30 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.700024

prev\_time=-28306 this\_time=-28306

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:10:07,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 bc 03 98 bc 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.000000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=101

rssi=71.500000 dist=43 return=101

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 65 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 4c 00 75 00 00 40 19 03 29 15 10 08 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 38 35 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 30 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.720133

prev\_time=-28306 this\_time=-28305

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682285N,126.710480E,0,19-▒3-29 15:10:08,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682285

jingdu = 126710480

gps\_info[0][0] = 101.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 49 00 75 00 00 40 19 03 29 15 10 04 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 30 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.909911

prev\_time=-28305 this\_time=-28303

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:04,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b9 03 98 b5 03 98 b9 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.500000 dist=45 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b9 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.750000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b8 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.750000 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 76

09 32 95 98 00 03 98 d0 c1 36 4d 00 75 00 00 40 19 03 29 15 10 15 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 82 33 2d 32 39 20 31 35 3a 31 30 3a 31 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02 03

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=6.230063

prev\_time=-28303 this\_time=-28297

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:15,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 ba 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.333333 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bb 03 98 ba 03 98 bb 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.000000 dist=42 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 ba 03 98 b1 03 98 b3 03 98 b3 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=69.000000 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 50 00 75 00 00 40 19 03 29 15 10 22 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 32 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=6.000023

prev\_time=-28297 this\_time=-28291

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:22,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 4f 00 75 00 00 40 19 03 29 15 10 19 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 31 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.500074

prev\_time=-28291 this\_time=-28290

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:19,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b5 03 98 b4 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=76.500000 dist=49 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b3 03 98 b3 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=76.000000 dist=49 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 51 00 75 00 00 40 19 03 29 15 10 23 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 32 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.779747

prev\_time=-28290 this\_time=-28289

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:23,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b5 03 98 b5 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=75.000000 dist=48 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 52 00 75 00 00 40 19 03 29 15 10 24 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 32 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.830261

prev\_time=-28289 this\_time=-28288

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:24,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b5 03 98 b5 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=75.250000 dist=48 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b6 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=75.000000 dist=48 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 53 00 75 00 00 40 19 03 29 15 10 27 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 32 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.390035

prev\_time=-28288 this\_time=-28286

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:27,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b3 03 98 b4 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=74.333333 dist=47 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b2 03 98 b7 03 98 b4 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=75.750000 dist=48 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b4 03 98 b7 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=75.000000 dist=48 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 55 00 75 00 00 40 19 03 29 15 10 32 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 33 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=4.899686

prev\_time=-28286 this\_time=-28281

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:32,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b6 03 98 b5 03 98 b4 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=75.500000 dist=48 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 54 00 75 00 00 40 19 03 29 15 10 29 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 32 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.949993

prev\_time=-28281 this\_time=-28280

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:29,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b4 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=74.750000 dist=47 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 b4 03 98 b6 03 98 b3 03 98 b3 03 98 b2

save\_msg datalength = 10

ee 03 98 b1 03 98 b4 03 98 b4 03 98 b5 03 98 b2

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=74.500000 dist=47 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b7 03 98 b4 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=75.666667 dist=48 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 57 00 75 00 00 40 19 03 29 15 10 37 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 33 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=4.070081

prev\_time=-28280 this\_time=-28276

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:37,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b8 03 98 b5 03 98 b6 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=76.000000 dist=49 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 bb 03 98 b9 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=72.500000 dist=45 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 58 00 75 00 00 40 19 03 29 15 10 38 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 33 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.901472

prev\_time=-28276 this\_time=-28275

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:38,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 ba 03 98 b9 03 98 b9 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.666667 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b6 03 98 b9 03 98 b7 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.333333 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 59 00 75 00 00 40 19 03 29 15 10 39 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 33 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.098472

prev\_time=-28275 this\_time=-28274

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:39,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 ba 03 98 b8 03 98 bb 03 98 bc 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=71.666667 dist=44 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bd 03 98 ba 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.500000 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 5a 00 75 00 00 40 19 03 29 15 10 40 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 34 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.200033

prev\_time=-28274 this\_time=-28273

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:40,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bb 03 98 bc 03 98 ba 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=68.666667 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 bb 03 98 bd 03 98 bb 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=69.000000 dist=40 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 5b 00 75 00 00 40 19 03 29 15 10 41 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 34 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.910012

prev\_time=-28273 this\_time=-28272

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:41,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b5 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=70.750000 dist=43 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b5 03 98 b4 03 98 b3 03 98 b2 03 98 b5

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b3 03 98 b4 03 98 b7 03 98 b8 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=73.500000 dist=46 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 5d 00 75 00 00 40 19 03 29 15 10 45 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 38 30 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 34 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=4.160163

prev\_time=-28272 this\_time=-28268

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710480E,0,19-▒3-29 15:10:45,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710480

gps\_info[0][0] = 100.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b1 03 98 b4 03 98 b4 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=74.666667 dist=47 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b7 03 98 b5 03 98 b4 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=76.000000 dist=49 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 b6 03 98 b7 03 98 b5 03 98 b6 03 98 b3

save\_msg datalength = 10

ee 03 98 b3 03 98 b2 03 98 b3 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=100

rssi=76.250000 dist=49 return=100

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 64 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 5e 00 75 00 00 40 19 03 29 15 10 47 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 34 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=5.659887

prev\_time=-28268 this\_time=-28262

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:10:47,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 60 00 75 00 00 40 19 03 29 15 10 51 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 35 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.199977

prev\_time=-28262 this\_time=-28262

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:10:51,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b8 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.750000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b7 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.333333 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b4 03 98 b4 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.500000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 62 00 75 00 00 40 19 03 29 15 10 57 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 30 3a 35 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=5.650007

prev\_time=-28262 this\_time=-28257

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:10:57,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b5 03 98 b4 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.500000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b4 03 98 b6 03 98 b8 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 ba 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.333333 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b4 03 98 b5 03 98 b4 03 98 b4 03 98 b5

save\_msg datalength = 10

ee 03 98 b5 03 98 b4 03 98 b7 03 98 b5 03 98 b1

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 67 00 75 00 00 40 19 03 29 15 11 17 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 31 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=32.810053

prev\_time=-28257 this\_time=-28224

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:17,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.666667 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b6 03 98 b5 03 98 b4 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 87

03 98 b6 03 98 b5 03 98 b8 03 98 ba 03 98 b8 79 7e 78 09 32 95 98 00 03 98 d0 c1 36 6a 00 75 00 00 40 19 03 29 15 11 30 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 33 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 ba 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.666667 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 bb 03 98 bb 03 98 bb 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.250000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 ba 03 98 bb 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=69.000000 dist=40 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b9 03 98 bb 03 98 b8 03 98 b9 03 98 b9

save\_msg datalength = 10

ee 03 98 b6 03 98 b9 03 98 bb 03 98 bb 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.666667 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 6c 00 75 00 00 40 19 03 29 15 11 34 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 33 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=5.070003

prev\_time=-28224 this\_time=-28219

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:34,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=69.500000 dist=41 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b2 03 98 b3 03 98 b5 03 98 b5 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 b7 03 98 b7 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 6d 00 75 00 00 40 19 03 29 15 11 36 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 33 36 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.689796

prev\_time=-28219 this\_time=-28217

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:36,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b8 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 6e 00 75 00 00 40 19 03 29 15 11 37 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 33 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.200153

prev\_time=-28217 this\_time=-28216

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:37,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b4 03 98 b4 03 98 b4 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.250000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b3 03 98 b6 03 98 b5 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.000000 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b3 03 98 b3 03 98 b6 03 98 b5 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.666667 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b8 03 98 b6 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.333333 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 70 00 75 00 00 40 19 03 29 15 11 42 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 34 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=4.429899

prev\_time=-28216 this\_time=-28211

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:42,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b6 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.750000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b8 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 71 00 75 00 00 40 19 03 29 15 11 43 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 34 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.470025

prev\_time=-28211 this\_time=-28210

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:43,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b9 03 98 b8 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.500000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 72 00 75 00 00 40 19 03 29 15 11 44 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 34 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.902697

prev\_time=-28210 this\_time=-28209

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:44,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.333333 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 73 00 75 00 00 40 19 03 29 15 11 45 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 34 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.697300

prev\_time=-28209 this\_time=-28208

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:45,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b7 03 98 b8 03 98 b8 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b5 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.500000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b9 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.500000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 75 00 75 00 00 40 19 03 29 15 11 47 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 34 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.810028

prev\_time=-28208 this\_time=-28207

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:47,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 76

09 32 95 98 00 03 98 d0 c1 36 76 00 75 00 00 40 19 03 29 15 11 48 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 82 33 2d 32 39 20 31 35 3a 31 31 3a 34 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.250137

prev\_time=-28207 this\_time=-28205

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:48,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b6 03 98 b5 03 98 b4 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b6 03 98 b6 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.750000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 77 00 75 00 00 40 19 03 29 15 11 49 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 34 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.999896

prev\_time=-28205 this\_time=-28204

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:49,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b6 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 74 00 75 00 00 40 19 03 29 15 11 46 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 34 36 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.650037

prev\_time=-28204 this\_time=-28204

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:46,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 78 00 75 00 00 40 19 03 29 15 11 50 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 35 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.050505

prev\_time=-28204 this\_time=-28204

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:50,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b9 03 98 ba 03 98 ba 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.000000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 79 00 75 00 00 40 19 03 29 15 11 51 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 35 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.199459

prev\_time=-28204 this\_time=-28202

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:51,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b7 03 98 b4 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=70.000000 dist=42 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b2 03 98 b4 03 98 b6 03 98 b8 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.333333 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 76

09 32 95 98 00 03 98 d0 c1 36 7a 00 75 00 00 40 19 03 29 15 11 52 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 82 33 2d 32 39 20 31 35 3a 31 31 3a 35 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02 03

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.050039

prev\_time=-28202 this\_time=-28200

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:52,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b6 03 98 b7 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b2 03 98 b3 03 98 b6 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.500000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b3 03 98 b5 03 98 b6 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=77.250000 dist=50 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 7b 00 75 00 00 40 19 03 29 15 11 54 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 31 3a 35 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.060027

prev\_time=-28200 this\_time=-28198

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:11:54,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b1 03 98 b5 03 98 b5 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b4 03 98 b7 03 98 b7 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.750000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b6 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 7e 00 75 00 00 40 19 03 29 15 12 01 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 30 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=6.389887

prev\_time=-28198 this\_time=-28192

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:01,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b4 03 98 b6 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b4 03 98 b3 03 98 b4 03 98 b2

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b4 03 98 b5 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.333333 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b9 03 98 b5 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.500000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b5 03 98 b5 03 98 b5 03 98 b5 03 98 b4

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 80 00 75 00 00 40 19 03 29 15 12 13 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 31 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=12.649990

prev\_time=-28192 this\_time=-28179

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:13,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b3 03 98 b5 03 98 b7 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.500000 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 81 00 75 00 00 40 19 03 29 15 12 15 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 31 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.999963

prev\_time=-28179 this\_time=-28178

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:15,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b5 03 98 b5 03 98 b4 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.666667 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b2 03 98 b5 03 98 b5 03 98 b5 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.250000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 82 00 75 00 00 40 19 03 29 15 12 17 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 31 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.110059

prev\_time=-28178 this\_time=-28176

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:17,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b7 03 98 b7 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b7 03 98 b7 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.500000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b7 03 98 b7 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.333333 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 ba 03 98 b5 03 98 b7 03 98 ba 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 ba 03 98 b8 03 98 b2

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.250000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 85 00 75 00 00 40 19 03 29 15 12 27 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 32 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=9.679994

prev\_time=-28176 this\_time=-28166

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:27,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.500000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b4 03 98 b5 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 86 00 75 00 00 40 19 03 29 15 12 27 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 32 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.361176

prev\_time=-28166 this\_time=-28165

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:27,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 bc 03 98 ba 03 98 bc

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 bd 03 98 bc 03 98 b9 03 98 b2 03 98 b6

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 84 00 75 00 00 40 19 03 29 15 12 25 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 32 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.688834

prev\_time=-28165 this\_time=-28163

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:25,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b5 03 98 b6 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=68.500000 dist=40 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 83 00 75 00 00 40 19 03 29 15 12 18 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 31 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.090027

prev\_time=-28163 this\_time=-28161

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:18,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b3 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.750000 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b7 03 98 b6 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 88 00 75 00 00 40 19 03 29 15 12 33 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 33 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.909963

prev\_time=-28161 this\_time=-28160

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:33,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b8 03 98 b2 03 98 b1 03 98 b2

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.500000 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 8a 00 75 00 00 40 19 03 29 15 12 35 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 33 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.500135

prev\_time=-28160 this\_time=-28158

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:35,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b4 03 98 b6 03 98 b5 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=77.500000 dist=51 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b4 03 98 b5 03 98 b3 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.750000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 b4 03 98 b4 03 98 b4 03 98 b3 03 98 b1

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b1 03 98 b2 03 98 b2 03 98 b2 03 98 b2

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.333333 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b5 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=78.000000 dist=51 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 8d 00 75 00 00 40 19 03 29 15 12 48 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 34 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=12.419972

prev\_time=-28158 this\_time=-28145

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:48,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b2 03 98 b4 03 98 b5 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.750000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b7 03 98 b6 03 98 b7 03 98 b7 03 98 b5

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b7 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.250000 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 8f 00 75 00 00 40 19 03 29 15 12 49 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 34 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.599948

prev\_time=-28145 this\_time=-28144

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:49,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b5 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b7 03 98 b7 03 98 b6 03 98 b4 03 98 b3

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 8c 00 75 00 00 40 19 03 29 15 12 39 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 33 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.349987

prev\_time=-28144 this\_time=-28142

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:39,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b5 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.666667 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 91 00 75 00 00 40 19 03 29 15 12 52 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 35 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800013

prev\_time=-28142 this\_time=-28141

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:52,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b4 03 98 b4 03 98 b5 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b6 03 98 b6 03 98 b5 03 98 b7 03 98 b5

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b2 03 98 b3 03 98 b7 03 98 b7 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.666667 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 ba 03 98 b9 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.666667 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 93 00 75 00 00 40 19 03 29 15 12 55 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 35 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.209952

prev\_time=-28141 this\_time=-28139

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:55,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 94 00 75 00 00 40 19 03 29 15 12 55 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 35 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.809952

prev\_time=-28139 this\_time=-28138

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:55,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b6 03 98 b3

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.666667 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b2 03 98 b5 03 98 b8 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.250000 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 95 00 75 00 00 40 19 03 29 15 12 56 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 35 36 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.080135

prev\_time=-28138 this\_time=-28137

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:56,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.500000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 96 00 75 00 00 40 19 03 29 15 12 57 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 35 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.379876

prev\_time=-28137 this\_time=-28135

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:57,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b9 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b7 03 98 b6 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.750000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 97 00 75 00 00 40 19 03 29 15 12 59 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 32 3a 35 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.409971

prev\_time=-28135 this\_time=-28134

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:12:59,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b6 03 98 b6 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 98 00 75 00 00 40 19 03 29 15 13 00 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 30 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.860136

prev\_time=-28134 this\_time=-28133

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:00,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b6 03 98 b5 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.500000 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b3 03 98 b4 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 b2 03 98 b2 03 98 b4 03 98 b4 03 98 b4

save\_msg datalength = 10

ee 03 98 b7 03 98 b5 03 98 b4 03 98 b5 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.250000 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b7 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.666667 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 9b 00 75 00 00 40 19 03 29 15 13 04 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 30 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=4.250547

prev\_time=-28133 this\_time=-28129

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:04,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b6 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b6 03 98 b6 03 98 b6 03 98 b6 03 98 b5

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 99 00 75 00 00 40 19 03 29 15 13 02 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 30 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.399381

prev\_time=-28129 this\_time=-28127

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:02,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b6 03 98 b6 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b6 03 98 b6 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 9d 00 75 00 00 40 19 03 29 15 13 07 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 30 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.100099

prev\_time=-28127 this\_time=-28126

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:07,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b4 03 98 b4 03 98 b5 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.333333 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b6 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.250000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b6 03 98 b7 03 98 b5 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.250000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 9e 00 75 00 00 40 19 03 29 15 13 08 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 30 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.100040

prev\_time=-28126 this\_time=-28125

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:08,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b7 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b6

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a0 00 75 00 00 40 19 03 29 15 13 10 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.999901

prev\_time=-28125 this\_time=-28123

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:10,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b7 03 98 b6 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.250000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b6 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.750000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a1 00 75 00 00 40 19 03 29 15 13 11 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800009

prev\_time=-28123 this\_time=-28122

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:11,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b6 03 98 b6 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a2 00 75 00 00 40 19 03 29 15 13 12 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800015

prev\_time=-28122 this\_time=-28122

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:12,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b6 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a3 00 75 00 00 40 19 03 29 15 13 13 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.500008

prev\_time=-28122 this\_time=-28120

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:13,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b4 03 98 b3 03 98 b3 03 98 b4 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a4 00 75 00 00 40 19 03 29 15 13 14 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.099916

prev\_time=-28120 this\_time=-28119

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:14,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b5 03 98 b4 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.250000 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a5 00 75 00 00 40 19 03 29 15 13 15 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800005

prev\_time=-28119 this\_time=-28118

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:15,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b3 03 98 b5 03 98 b5 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b3 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.250000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a6 00 75 00 00 40 19 03 29 15 13 16 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 36 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800134

prev\_time=-28118 this\_time=-28117

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:16,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b4 03 98 b3 03 98 b6 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.000000 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a7 00 75 00 00 40 19 03 29 15 13 17 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.999856

prev\_time=-28117 this\_time=-28116

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:17,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b5 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

xread n\_read = = 0save\_msg datalength = 0f

03 98 b5 03 98 b4 03 98 b6 03 98 b6 03 98 b5

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b4 03 98 b4 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 a9 00 75 00 00 40 19 03 29 15 13 19 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 31 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.999999

prev\_time=-28116 this\_time=-28114

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:19,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b5 03 98 b3 03 98 b4 03 98 b7 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.750000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 aa 00 75 00 00 40 19 03 29 15 13 20 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.700016

prev\_time=-28114 this\_time=-28114

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:20,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b4 03 98 b6 03 98 b4 03 98 b5 03 98 b2

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.250000 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b4 03 98 b3 03 98 b8 03 98 b4

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.333333 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 ab 00 75 00 00 40 19 03 29 15 13 20 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.902738

prev\_time=-28114 this\_time=-28113

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:20,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b5 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=76.000000 dist=49 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b4 03 98 b4 03 98 b5 03 98 b6 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.333333 dist=47 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b4 03 98 b8 03 98 b8 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.500000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b9 03 98 b9 03 98 b9 03 98 b9 03 98 b9

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.500000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b9 03 98 b9 03 98 b9 03 98 b9 03 98 b9

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 ae 00 75 00 00 40 19 03 29 15 13 23 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=3.127252

prev\_time=-28113 this\_time=-28110

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:23,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b9 03 98 bb 03 98 bb

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.000000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 ba 03 98 ba 03 98 ba 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=69.750000 dist=41 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 af 00 75 00 00 40 19 03 29 15 13 24 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.900093

prev\_time=-28110 this\_time=-28109

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:24,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 ac 00 75 00 00 40 19 03 29 15 13 21 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.799918

prev\_time=-28109 this\_time=-28108

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:21,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 76

09 32 95 98 00 03 98 d0 c1 36 b0 00 75 00 00 40 19 03 29 15 13 25 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 82 33 2d 32 39 20 31 35 3a 31 33 3a 32 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02 03

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.200268

prev\_time=-28108 this\_time=-28108

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:25,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 b1 00 75 00 00 40 19 03 29 15 13 27 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.599847

prev\_time=-28108 this\_time=-28106

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:27,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 b2 00 75 00 00 40 19 03 29 15 13 28 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.800010

prev\_time=-28106 this\_time=-28105

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:28,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 b3 00 75 00 00 40 19 03 29 15 13 29 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 32 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.999909

prev\_time=-28105 this\_time=-28104

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:29,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b7 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b7

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 b5 00 75 00 00 40 19 03 29 15 13 31 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 33 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.600354

prev\_time=-28104 this\_time=-28102

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:31,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b6 03 98 b6 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b7 03 98 b5 03 98 b7 03 98 b7 03 98 b5

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b7 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 b7 00 75 00 00 40 19 03 29 15 13 34 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 33 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.299631

prev\_time=-28102 this\_time=-28099

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:34,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b6 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b6 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 b8 00 75 00 00 40 19 03 29 15 13 35 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 33 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.899955

prev\_time=-28099 this\_time=-28098

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:35,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.500000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 b9 00 75 00 00 40 19 03 29 15 13 35 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 33 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.700101

prev\_time=-28098 this\_time=-28098

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:35,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b9 03 98 b8 03 98 b7 03 98 b5 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.500000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b9 03 98 bb 03 98 bb 03 98 ba 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.666667 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 87

03 98 ba 03 98 b7 03 98 b6 03 98 b7 03 98 b7 b4 7e 78 09 32 95 98 00 03 98 d0 c1 36 bb 00 75 00 00 40 19 03 29 15 13 37 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 33 37 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

save\_msg datalength = 10

ee 03 98 b5 03 98 b7 03 98 b7 03 98 b6 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=70.000000 dist=42 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b5 03 98 b7 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 bc 00 75 00 00 40 19 03 29 15 13 38 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 33 38 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=2.499853

prev\_time=-28098 this\_time=-28095

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:38,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b6 03 98 b6 03 98 b6 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.500000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 bd 00 75 00 00 40 19 03 29 15 13 39 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 33 39 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.900057

prev\_time=-28095 this\_time=-28094

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:39,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b6 03 98 b7 03 98 b5 03 98 b5 03 98 b6

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=74.000000 dist=46 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b8 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 be 00 75 00 00 40 19 03 29 15 13 40 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 34 30 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.100178

prev\_time=-28094 this\_time=-28093

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:40,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b7 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b7 03 98 b8 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 bf 00 75 00 00 40 19 03 29 15 13 41 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 34 31 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.101301

prev\_time=-28093 this\_time=-28092

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:41,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b7 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 c0 00 75 00 00 40 19 03 29 15 13 42 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 34 32 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.998511

prev\_time=-28092 this\_time=-28091

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:42,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 c1 00 75 00 00 40 19 03 29 15 13 43 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 34 33 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.900174

prev\_time=-28091 this\_time=-28090

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:43,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 c2 00 75 00 00 40 19 03 29 15 13 44 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 34 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=0.799914

prev\_time=-28090 this\_time=-28089

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:44,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b8 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 c3 00 75 00 00 40 19 03 29 15 13 45 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 34 35 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=1.100042

prev\_time=-28089 this\_time=-28088

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:45,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b7 03 98 b8 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b5 03 98 b8 03 98 b8 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.500000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b5 03 98 b7 03 98 ba

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 bb 03 98 ba 03 98 bb 03 98 ba 03 98 bb

save\_msg datalength = 10

ee 03 98 bc 03 98 bc 03 98 b7 03 98 ba 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.333333 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 c4 00 75 00 00 40 19 03 29 15 13 46 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 34 36 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=5.199983

prev\_time=-28088 this\_time=-28083

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:46,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

save\_msg datalength = 10

ee 03 98 b8 03 98 b8 03 98 b8 03 98 b8 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.750000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b8 03 98 b9 03 98 bb 03 98 ba 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=72.000000 dist=44 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

xread n\_read = = 0save\_msg datalength = 0f

03 98 b5 03 98 b5 03 98 b5 03 98 b7 03 98 b5

save\_msg datalength = 10

ee 03 98 b6 03 98 b5 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=71.000000 dist=43 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b4 03 98 b4 03 98 b5 03 98 b5 03 98 b5

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 75

09 32 95 98 00 03 98 d0 c1 36 c7 00 75 00 00 40 19 03 29 15 13 54 41 4c 30 30 30 35 00 35 39 c2 b7 00 c9 cf d0 d0 00 00 34 35 2e 36 38 32 32 37 34 4e 2c 31 32 36 2e 37 31 30 34 36 34 45 2c 30 2c 31 39 2d 81 33 2d 32 39 20 31 35 3a 31 33 3a 35 34 2c 30 2e 30 30 30 30 30 30 2c 33 33 2e 37 00 ba cd d0 cb c2 b7 00 30 2e 30 30 30 30 30 30 00 00 02 03 02

29ce4 29cee\*\*\*\*\*\*\*message ID 5009 recived from uart\*\*\*\*\*\*

write file end

queNo = 0

rssibuff[26][0] = 5

convert\_string start

diff\_time=3.790056

prev\_time=-28083 this\_time=-28079

4c 30 30 30 35 car No end

35 39 c2 b7 line info end

c9 cf d0 d0 service info end

driver info end

45.682274N,126.710464E,0,19-▒3-29 15:13:54,0.000000,33.7locate info end

WEIDU = 0.000000,JINGDU = 0.000000

weidu = 45682274

jingdu = 126710464

gps\_info[0][0] = 99.000000

hight = 0

30

speed=0

gps\_info[1][0] = 3.658294

gps\_info[3][0] = 0.000000

gps\_info[4][0] = 0.000000

gps\_info[5][0] = 0.000000

gps\_info[6][0] = 0.000000

33 33 direction=33

direction= 00 21

convert\_string end

info\_from\_service\_and\_send\_to\_uart

save\_msg datalength = 10

ee 03 98 b5 03 98 b6 03 98 b7 03 98 b7 03 98 b7

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=75.000000 dist=48 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

save\_msg datalength = 10

ee 03 98 b7 03 98 b2 03 98 b5 03 98 b7 03 98 b8

RSSI EE recived from uart

queueNo is 0

dist by gps7=99

rssi=73.000000 dist=45 return=99

flag = 06,

8=03,9=01

7e 0b ee 00 03 98 63 01 03 03 00

queueNo is 0

queueNo is 0

queueNo is 0

queueNo is 0

[1] + Stopped ./taxier

~ $